*Use at your own risk. The pilot must refer to the FAA approved documents for the*

 *correct information and is responsible for safe operation of aircraft*.

Emergency: Com 121.5 / Squawk 7700

Loss Com. Squawk 7600

KMAN ASOS:118.325 KEUL ASOS :135.07 KBOI ATIS:123.9

Big Sky App/Dep: 119.6 unless directed to 126.9 FSS BOI: 122.6

|  |
| --- |
| **Cessna 182P N9989E v1.6 7/31/2020** |
| **TAKEOFF**Normal: Rotate 60 MPH **Vy 89 MPH**  (85 mph @ 10,000’)Short/Soft: Flaps 20° **Vx 60 MPH** (64 mph @ 10,000’) |
| **CRUISE CLIMB 100 – 120 MPH****BEST GLIDE 80 MPH (flaps up)** |
| **>1000’ AGL** Oil Pres/Temp • Ammeter • Vacuum• MP **15”- 23”** • Prop **2200 -2450 RPM** |
| **CRUISE** • Max 75% power • Mixture LEAN to **peak EGT**, then ENRICH 125˚F rich of peak for Best power.• Heading Indicator **SET** • Cowl Flaps **CLOSED**• Routinely Check Gauges:• Oil Press/Temp • Ammeter • Landing Light **ON for Safety** |
| **LANDING** • Landing Light **ON**• Autopilot **OFF** • Carb Heat **ON** • Prop **FWD** • Cowl Flaps **CLOSED** • Fuel **BOTH** • Mixture **ENRICH**• Approach at **70-80 MPH** |
| **GO AROUND**• Full Throttle • Pitch up • Carb Heat **OFF** • Flaps retract to **20°**• Climbing & above ***80 MPH***, retract flaps • Cowl Flaps **OPEN** |
| **AFTER LANDING**Carb Heat **OFF** • Transponder **SBY** • Flaps **UP**Cowl Flaps **OPEN** • Mixture **LEAN** for taxi |
| **SHUTDOWN** Avionics/Lights **OFF** • Mixture **OFF** • Master **OFF** • Mags **OFF**Flight Plan **Closed** • Control Lock **Installed** •Pitot Tube Cover **Installed** |
| **POSTFLIGHT** • Hobbs & Tach Time **RECORDED** • Windows & Leading Edges **CLEANED**• Wheel Chocks **SET** • Seat Belts **SECURE** • Interior **CLEANED**• Airplane **LOCKED** • Flight Log **DATA** **ENTERED** • Flight Plan **CLOSED**• Hangar **SECURE** • Lights **OFF** • Doors **LOCKED** |
| *MPH***Vso 63****Vs1 68****Vfe 110****Va 2950 126****Va 2500 116****Va 2050 105****Vno 160****Vne 198** | Recommended Pattern Speeds/ Approx Pwr SettingsDownwind: 90 - 100 mph / 16“ MPAbeam: 85 - 90 mph / 13“ MP Base: 80 - 85 mph / 13“ MPFinal: 70 - 75 mph / 13“ MP (Full Flaps – No Flaps) |

*Use at your own risk. The pilot must refer to the FAA approved documents for the*

*correct information and is responsible for safe operation of aircraft*.

|  |
| --- |
| **Cessna 182P N9989E v1.6 7/31/2020** |
| PREFLIGHTPitot Tube Cover - REMOVEDGust Lock - REMOVEDHobbs – Record into Flight LogTach – Check < Oil Change TimeAvionics Master–OFFMaster - ONFlaps – Ck for Smooth OperationFuel Gauges – CHECKExterior Lights - CHECKInterior Lights – CHECKStall Horn - CHECKMaster – OFFBaggage Door – LOCKEDTires/Brakes – Press/Leaks(Main 42 psi - Nose 49 psi)Fuel Quantity & Caps secureOil level: 7 MIN / 8 MAX Qts. Oil Filler Cap – SecureNose strut, Cowl Flaps,Prop & Spinner - InspectStatic Ports-ClearCheck Fuel level/Caps/DrainEngine Fuel Strainer-DrainFinal Walk / Look AroundSTARTSeats – LOCKEDSeat Belts – FASTENEDPassenger BriefingCowl Flaps – OPENElevator / Rudder Trim SetCircuit Breakers – INAvionics – OFFAutoPilot –OFF (is off by default)Mixture – RICHCarb Heat – COLDPrime – As Required (max 3)Throttle – OPEN ½ InchYell - Clear Prop | Brakes – Set/HeldMaster – ONBeacon – ONEngage Starter (max 20 sec crank if no start)AFTER STARTThrottle – 1000 RPMOil Pressure– in green < 30 secondsFlaps – UPMixture – LEAN FOR TAXIAvionics Master – ONTaxi Lights - ONTransponder – ALTRUNUPDoors & Windows – LATCHEDControls – FREE & CORRECTFlaps – UPTrim – Elevator & Rudder TAKEOFFThrottle – 1700 RPMMixture – FULL RICH (Lean for Best power above 5,000’ DA)Mags (drop< 125, difference ea <50)Prop – Cycle 3 XCarb Heat – TESTAmmeter - ChargingLow Voltage Light - Out Throttle – 1000 RPMInstruments – CHECK/SETGarmin G5 baro pressure set/referenced to conventional Altimeter Seat Belts – SECURECOM – First Freq. 122.7 KMANNAV – First Freq. - 113.3 BOI VOR OBS – SETCharts & Log – READYHeadset – ON |
| **BEFORE TAKEOFF - Clearing** circle for Pattern Traffic • What is your **ABORT** Plan?Flaps **UP** or 20° • Carb Heat **OFF** • Transponder **ALT** • Lights/Strobes **ON** • Prop **FWD** • Cowl Flaps **OPEN** • Headset **ON** |

Emergency: Com 121.5 / Squawk 7700

Loss Com. Squawk 7600

KMAN ASOS:118.325 KEUL ASOS :135.07 KBOI ATIS:123.9

Big Sky App/Dep: North 126.9 / South 119.6