*Use at your own risk. The pilot must refer to the FAA approved documents for the*

 *correct information and is responsible for safe operation of aircraft*.

|  |
| --- |
| **Cessna 182Q N121M v1.3 5/20/2021** |
| **TAKEOFF**Normal: Rotate 50 Kts **Vy 78 Kts**  (72 kts @ 10,000’)Short/Soft: Flaps 20° **Vx 50 Kts** (58 kts @ 10,000’) |
| **CRUISE CLIMB 85 – 95 Kts****BEST GLIDE 70 Kts (flaps up)** |
| **>1000’ AGL** Oil Pres/Temp • Ammeter • Vacuum• MP **15”- 23”** • Prop **2100 -2400 RPM** |
| **CRUISE** • Max 75% power • Mixture LEAN to **peak EGT**, then ENRICH 50˚F rich of peak for Best power.• Cowl Flaps **As Required**• Routinely Check Gauges:• Oil Press/Temp • Ammeter • Landing Light **On for Safety** |
| **LANDING** • Landing Light **ON** • Auto-Pilot **OFF** • Elec. Trim **OFF**• Carb Heat **ON** • Prop **FWD** • Cowl Flaps **CLOSED** • Fuel **BOTH** • Mixture **ENRICH**• Approach at **60-70 Kts** |
| **GO AROUND**• Full Throttle • Pitch up • Carb Heat **OFF** • Flaps retract to **20°**• Climbing & above ***55 kts***, retract flaps • Cowl Flaps **OPEN** |
| **AFTER LANDING**Carb Heat **OFF** • Transponder **SBY** • Flaps **UP**Cowl Flaps **OPEN** • Mixture **LEAN** for taxi |
| **SHUTDOWN**Avionics/Lights **OFF** • Mixture **OFF** • Mags **OFF**• Master **OFF**Flight Plan **Closed** • Control Lock **Installed** Pitot Tube Cover - **Installed**  |
| **POSTFLIGHT** • Hobbs & Tach Times **RECORDED** • Windows & Leading Edges **CLEANED**Seat Belts **SECURE** • Interior **CLEANED** • Airplane **LOCKED**Wheel Chocks **SET**• Tow Bar **REMOVED** Flight Log **ENTERED** • Hangar **SECURE** • Lights **OFF**  |
|  *Kts***Vso 38****Vs1 53****Vfe 95****Va 2950 111****Va 2500 102****Va 2050 93****Vno 143****Vne 179** | Recommended Pattern Speeds/ Approx Pwr SettingsDownwind: 85 - 90 Kts / 16“ MPAbeam: 75 - 80 Kts / 13“ MP Base: 70 - 75 Kts / 13“ MPFinal: 55 - 65 Kts / 13“ MP (Full Flaps – No Flaps) |

Emergency: Com 121.5 / Squawk 7700

Loss Com. Squawk 7600

KMAN ASOS:118.325 KEUL ASOS :135.07 KBOI ATIS:123.9

Big Sky App/Dep: 119.6 unless directed to 126.9 FSS BOI: 122.6

*Use at your own risk. The pilot must refer to the FAA approved documents for the*

*correct information and is responsible for safe operation of aircraft*.

|  |
| --- |
| **Cessna 182Q N121M v1.3 5/20/2021** |
| PREFLIGHTPitot Tube Cover - REMOVEDGust Lock - REMOVEDHobbs – Match Flight LogAvionics Master–OFFMaster – ONTach – Check < Oil Change TimeFlaps – Ck for Smooth Operation and Aileron drop with flaps. Fuel Gauges – CHECKExterior Lights – (Beacon on Avionics Master) CHECKInterior Lights – CHECKStall Horn - CHECKMaster – OFFBaggage Door – LOCKEDTires/Brakes – Press/Leaks(Main 25 psi - Nose 25 psi)Fuel Quantity & Caps secureCareful with VG’s when Fueling.Not Airworthy if more than 5 VG’s are missing – Ground PlaneOil level: 7 MIN / 8 MAX Qts. Oil Filler Cap – Secure Nose strut, Cowl Flaps,Prop & Spinner - InspectStatic Port(s)-ClearCheck Fuel level/Caps/DrainEngine Fuel Strainer-DrainFinal Walk/Look Around/Tow BarSTARTSeats–LOCKED (Pilot Seat Lock)Seat Belts – FASTENEDPassenger BriefingCowl Flaps – OPENElevator / Rudder Trim SetCircuit Breakers – INAvionics – OFFMixture – RICHCarb Heat – COLDPrime – As Required (max 3x)Throttle – OPEN ~ ½ InchYell - Clear Prop | Brakes – Set/HeldMaster – ONBeacon – ONEngage Starter (max 20 sec crank if no start)AFTER STARTThrottle – 1000 RPMOil Pressure– in green < 30 secondsFlaps – UPMixture – LEAN FOR TAXIAvionics Master – ONTaxi/Landing Lights - ONTransponder – ALTRUNUPDoors & Windows – LATCHEDControls – FREE & CORRECTFlaps – UPTrim – Elevator & Rudder TAKEOFFThrottle – 1700 RPMMixture – FULL RICH (Lean for best power above 5,000’ DA)Mags (drop< 125, difference ea <50)Prop – Cycle 3 XVacuum Check – In the GreenCarb Heat – TESTAmmeter - ChargingLow Voltage Light - Out Throttle – 1000 RPMInstruments – CHECK/SETSeat Belts – SECURECOM – First Freq. 122.7 KMANKMAN ASOS:118.325 NAV – First Freq. - 113.3 BOI VOR OBS – SETCharts & Log – READYHeadset – ONAuto-Pilot OFF Elec. Trim OFF |
| **BEFORE TAKEOFF - Clearing** circle for Pattern Traffic • What is your **ABORT** Plan?Flaps **UP** or 20° • Carb Heat **OFF** • Transponder **ALT** • Lights/Strobes **ON** • Prop **FWD** • Cowl Flaps **OPEN** • Headset **ON** |